**Publication on the CAN network of the sw version of the display**

When connecting to the CAN network with the kvaser tool, the sw version is shown in the fifth byte of the message with ID 630.

The figure below highlights the number 16 which corresponds to version 1.6.

